Dokumentáció Halász Noel

|  |  |
| --- | --- |
| Részleg név | IP cím |
| IT, pénzügy | 192.168.1.0 |
| HR és ügyfélszolgálat | 192.168.1.64 |
| Recepció | 192.168.1.128 |

|  |  |  |
| --- | --- | --- |
| Hálózat | DHCP címtartomány | Kizárt cím |
| Recepció | 192.168.1.0 | 192.168.1.1-192.168.1.5 |
| HR és ügyfélszolgálat | 192.168.1.64 | 192.168.1.129-192.168.1.130 |
| IT, pénzügy | 192.168.1.128 | 192.168.1.65-192.168.1.70 |

Home Routerek nevei jelszavai:

|  |  |  |
| --- | --- | --- |
| Router név | SSID | PASS |
| Recepcio R | recepcio | 123456789 |
| HR és ügyfélszolgálat R | hr | 123456789 |
| IT R | it | 123456789 |

|  |  |  |
| --- | --- | --- |
| VLAN | Részleg név | IP cím |
| 10 | Recepció | 192.168.1.0/26 |
| 20 | IT | 192.168.1.64/26 |
| 30 | HR és ügyfélszolgálat | 192.168.1.128/26 |

|  |
| --- |
| Router  hostname ROUTER  ip dhcp excluded-address 192.168.1.1 192.168.1.5  ip dhcp excluded-address 192.168.1.62  ip dhcp excluded-address 192.168.1.129 192.168.1.130  ip dhcp excluded-address 192.168.1.190  ip dhcp excluded-address 192.168.1.65 192.168.1.70  ip dhcp excluded-address 192.168.1.126  ip dhcp pool recepcio  network 192.168.1.0 255.255.255.192  default-router 192.168.1.1  ip dhcp pool hr  network 192.168.1.128 255.255.255.192  default-router 192.168.1.129  ip dhcp pool it  network 192.168.1.64 255.255.255.192  default-router 192.168.1.65  ip cef  no ipv6 cef  license udi pid CISCO2911/K9 sn FTX1524SGIX-  spanning-tree mode pvst  interface GigabitEthernet0/0  no ip address  duplex auto  speed auto  interface GigabitEthernet0/0.10  encapsulation dot1Q 10  ip address 192.168.1.1 255.255.255.192  interface GigabitEthernet0/0.20  encapsulation dot1Q 20  ip address 192.168.1.65 255.255.255.192  interface GigabitEthernet0/0.30  encapsulation dot1Q 30  ip address 192.168.1.129 255.255.255.192  interface GigabitEthernet0/1  no ip address  duplex auto  speed auto  shutdown  interface GigabitEthernet0/2  no ip address  duplex auto  speed auto  shutdown  interface Vlan1  no ip address  shutdown  ip classless  ip flow-export version 9  line con 0  line aux 0  line vty 0 4  login  end |

|  |
| --- |
| Switch  hostname SWITCH  spanning-tree mode pvst  spanning-tree extend system-id  interface FastEthernet0/1  switchport access vlan 10  switchport mode access  interface FastEthernet0/2  switchport access vlan 20  switchport mode access  interface FastEthernet0/3  switchport access vlan 30  switchport mode access  interface FastEthernet0/4  switchport access vlan 10  switchport mode access  interface FastEthernet0/5  switchport access vlan 30  switchport mode access  interface FastEthernet0/6  switchport access vlan 20  switchport mode access  interface FastEthernet0/7  switchport access vlan 20  switchport mode access  interface FastEthernet0/8  switchport access vlan 30  switchport mode access  interface FastEthernet0/9  switchport access vlan 10  switchport mode access  interface FastEthernet0/10  interface FastEthernet0/11  interface FastEthernet0/12  interface FastEthernet0/13  interface FastEthernet0/14  interface FastEthernet0/15  interface FastEthernet0/16  interface FastEthernet0/17  interface FastEthernet0/18  interface FastEthernet0/19  interface FastEthernet0/20  interface FastEthernet0/21  interface FastEthernet0/22  interface FastEthernet0/23  interface FastEthernet0/24  interface GigabitEthernet0/1  switchport mode trunk  interface GigabitEthernet0/2  interface Vlan1  no ip address  shutdown  line con 0  line vty 0 4  login  line vty 5 15  login  end |

A képen szöveg, képernyőkép, diagram, sor látható

Automatikusan generált leírás