Source

**Forgalomirányítók:**

*R-BP:*

hostname BUDAPEST

enable secret 5 $1$mERr$.sBeQ4nkWBbwCNrfZ7P97/

enable password GDszeged22

no ip cef

no ipv6 cef

ip ssh version 2

ip domain-name cisco.com

interface GigabitEthernet7/0

ip address 185.62.128.1 255.255.255.128

duplex auto

speed auto

interface GigabitEthernet8/0

ip address 8.8.0.1 255.255.0.0

duplex auto

speed auto

interface GigabitEthernet9/0

ip address 185.62.128.225 255.255.255.252

ip classless

ip route 0.0.0.0 0.0.0.0 8.8.0.0

ip flow-export version 9

line con 0

line aux 0

line vty 0 4

login local

transport input ssh

line vty 5 15

login local

transport input ssh

end

*R-SZEGED:*

hostname R-SZEGED

enable secret 5 $1$mERr$.sBeQ4nkWBbwCNrfZ7P97/

no ip cef

no ipv6 cef

interface GigabitEthernet8/0

ip address 185.62.128.221 255.255.255.224

duplex auto

speed auto

interface GigabitEthernet9/0

ip address 185.62.128.10 255.255.255.252

ip classless

ip route 185.62.128.0 255.255.255.128 185.62.128.225

ip route 185.62.128.0 255.255.255.128 185.62.128.9

ip route 185.62.128.128 255.255.255.192 185.62.128.9

ip flow-export version 9

banner login ^CMagan terulet^C

banner motd ^CNapfeny varos koszont^C

line con 0

line aux

line vty 0 4

login

end

*R-KECSKEMET:*

hostname R-KECSKEMET

ip cef

no ipv6 cef

interface GigabitEthernet6/0

ip address 185.62.128.140 255.255.255.192

duplex auto

speed auto

interface GigabitEthernet7/0

ip address 185.62.128.226 255.255.255.252

interface GigabitEthernet8/0

ip address 185.62.128.9 255.255.255.252

interface GigabitEthernet9/0

ip address 185.62.128.229 255.255.255.252

router rip

ip classless

ip route 185.62.128.192 255.255.255.224 185.62.128.10

ip route 185.62.128.0 255.255.255.128 185.62.128.225

ip route 185.62.128.128 255.255.255.192 185.62.128.230

ip route 185.62.128.192 255.255.255.192 185.62.128.230

ip route 8.8.0.0 255.255.0.0 185.62.128.225

ip route 192.168.10.0 255.255.255.0 185.62.128.230

ip flow-export version 9

line con 0

line aux 0

line vty 0 4

login

end

*R-SZOLNOK:*

hostname R-SZOLNOK

no ip cef

no ipv6 cef

interface GigabitEthernet6/0

ip address 185.62.128.230 255.255.255.252

interface GigabitEthernet7/0

no ip address

duplex auto

speed auto

shutdown

interface GigabitEthernet8/0

ip address 192.168.10.1 255.255.255.0

duplex auto

speed auto

interface GigabitEthernet9/0

no ip address

duplex auto

speed auto

shutdown

ip classless

ip route 185.62.128.0 255.255.255.128 185.62.128.229

ip route 185.62.128.128 255.255.255.192 185.62.128.229

ip route 185.62.128.192 255.255.255.224 185.62.128.229

ip route 8.8.0.0 255.255.0.0 185.62.128.229

ip flow-export version 9

line con 0

line aux 0

line vty 0 4

login

end